- Main Page
- Related Pages
- Classes
- Files

- Class List
- Class Hierarchy
- Class Members

Public Attributes

# SCS::canAS_Data_t Union Reference

Union combining CAN Aerospace message data types. More...

`#include <canaerotypes.h>`

List of all members.

## Public Attributes
float | flt
| float according to IEEE
uint32_t | uLong
| Unsigned 32 bit integer.
int32_t | sLong
| Signed 32 bit integer.
uint16_t | uShort [2]
| 2 x unsigned 16 bit integer.
int16_t | sShort [2]
| 2 x signed 16 bit integer.
uint8_t | uChar [4]
| 4 x unsigned 8 bit integer.
int8_t | sChar [4]
| 4 x signed 8 bit integer.
char | aChar [4]
| 4 x unsigned ASCII character.

## Detailed Description

Union combining CAN Aerospace message data types.

This union holds all possible data that can be transmitted in the bytes 4-7 of a CAN Aerospace message. Binary data types will be handled through their unsigned variants.

The documentation for this union was generated from the following file:

- canaerotypes.h